**HVAC Balanced Ambient Calorimeter**

* Tescor’s Balanced Ambient Calorimeters are designed to be supplied as calibrated room type or full balanced ambient with a conditioned annular space around the test room. Room temperature and humidity conditions are precisely and accurately controlled. All power inputs to the inner rooms and the test unit are measured and balanced. The calorimeters are provided with a fully automatic, computerized data acquisition and control system.
* Available Options:
  + Automated Pressure Equalizer
  + Outdoor Room Controlled Annular Space
  + Heating Capacity Test Capability without reversing UUT mounting
  + Air-Flow Code Tester for Airflow Measurement