**HVAC Trailer Mounted Conditioning Chamber**

* + Tescor’s Trailer-Mounted Conditioning Chambers are specially designed to provide a Test Space at precisely controlled temperature conditions for use in Test Product Temperature conditioning at different locations. Our units are designed for maximum accuracy, reliability, stability and ease of transport. The Trailer-Mounted Conditioning Chamber system includes a mechanical service room housing all the support refrigeration and heating equipment and control panel. The TMCC is completely self-sufficient when connected to the local power source using the retractable power cable.
  + Trailer-Mounted Conditioning Chambers have been widely utilized in the following applications:
    - Automotive Climate Control Component Development
    - Ammunition Temperature Conditioning
    - Missile Temperature Conditioning

**Specifications:**

|  |  |
| --- | --- |
| **Ambient Air**  **Conditions** | **Chamber Controlled**  **Conditions** |
| Dry Bulb Temperature | Dry Bulb Temperature |
| -40°F to 120°F | -67°F to 170°F ± 2°F |